**PPE (PERSONAL PROTECTIVE EQUIPMENT)**

This is the minimum PPE requirement you are expected to carry.

|  |  |
| --- | --- |
| Item | Description |
| 1 | Coveralls |
| 2 | Safety/Protective Helmet |
| 3 | Ear Muffs |
| 4 | Safety Glasses – Clear |
| 5 | High-Visibility Vest |
| 6 | Ear Plugs |
| 7 | Work Gloves |
| 8 | Safety Boots – Pair |
| 9 | Safety Harness – 3-Point c/w shock absorbing lanyard with 60mm snap hook |

**General PPE Advice:**

You are responsible for maintaining your PPE in good condition and servicing in line with manufacturer’s recommendations as a minimum. Faulty equipment should be reported to your FW Marsh manager and not used with immediate effect. Unless confirmed as not required prior to mobilisation, you are required to take your PPE with you for all assignments.

Certain job tasks may require additional PPE; these items will be supplied at work site as needed. If you have not received training on a particular PPE item, contact your supervisor immediately prior to performing the task.

|  |  |
| --- | --- |
| PPE Item | Required when (examples): |
| Safety Glasses and Face Shield | * Steam Cleaning * Chemical handling (closed systems/containers) * Spray painting * Flooding stator (painting) * Generator taping/tying * Bucket removal/peening |
| Safety Goggles and Face Shield | * Using cut-off wheel * Cutting causing airborne particles * Grinding metal * Abrasive grinding * Metal removal with burrs * Use of chop saw * Chemical handling (open system/containers) |